%%{
    let options = args.options;

    exampleType   = "input_interrupt";
    if(options && options.exampleType)
         exampleType = options.exampleType;

%%}
/*
 *  Copyright (C) 2018-2021 Texas Instruments Incorporated
 *
 *  Redistribution and use in source and binary forms, with or without
 *  modification, are permitted provided that the following conditions
 *  are met:
 *
 *    Redistributions of source code must retain the above copyright
 *    notice, this list of conditions and the following disclaimer.
 *
 *    Redistributions in binary form must reproduce the above copyright
 *    notice, this list of conditions and the following disclaimer in the
 *    documentation and/or other materials provided with the
 *    distribution.
 *
 *    Neither the name of Texas Instruments Incorporated nor the names of
 *    its contributors may be used to endorse or promote products derived
 *    from this software without specific prior written permission.
 *
 *  THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
 *  "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
 *  LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
 *  A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
 *  OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
 *  SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
 *  LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
 *  DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
 *  THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
 *  OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

#include <stdlib.h>
#include <drivers/hw_include/cslr_soc.h>
#include <drivers/gpio.h>
#include "ti_drivers_config.h"

/*
 * Board info
 */
% if ( exampleType == "input_interrupt" ) {
/* This is based on DMSC board config and core */
%if(args.project.board == "am263x-lp") {
#define BOARD_BUTTON_GPIO_INTR_NUM      (CSLR_R5FSS0_CORE0_INTR_GPIO_INTRXBAR_OUT_14)
#define BOARD_BUTTON_GPIO_SWITCH_NUM    (4)
%}
%else {
#define BOARD_BUTTON_GPIO_INTR_NUM      (CSLR_R5FSS0_CORE0_INTR_GPIO_INTRXBAR_OUT_14)
#define BOARD_BUTTON_GPIO_SWITCH_NUM    (1)
%}

void Board_gpioInit(void)
{
}

void Board_gpioDeinit(void)
{
}

uint32_t Board_getGpioButtonIntrNum(void)
{
    return (BOARD_BUTTON_GPIO_INTR_NUM);
}

uint32_t Board_getGpioButtonSwitchNum(void)
{
    return (BOARD_BUTTON_GPIO_SWITCH_NUM);
}
% }
