{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"flags":["formulas_cached_only"]}
["150 MHz"]
[null,"CPU Freq",{"v":150000000,"d":"1.50E+08"},null,null,"Inputs"]
[null,"Maximum Required Freq",{"v":10000,"d":"1.00E+04"},"BaseFreq",null,"Output information needed for configuration"]
[null,"Minimum Required Freq",50,null,null,"Information"]
[]
["FREQ_UTIME","Freq measurement rate (Hz)",100,"UTPRD","Unit Time period to be programmed for100Hz"]
[null,"Freq Resolution",50]
[null,"QEP Count at Max Freq",{"v":200,"d":"2.00E+02"},"freqScalar_fr"]
[]
["FREQ_PRD","QEP edges for avg time measurement(2^k)",4,"QCAPCTL.UPPS","Unit position prescalar to 1/4"]
[null,"Time for selected QEP edges at min RPM(s)",0.04,"T= edges/(2*Fmin)"]
[null,"QEP CAP clock to avoid overflow(Hz)",1638375,"Fcapmax=maxcnt/T"]
[null,"Minimum QEP Clock pre-scalar",{"v":91.55413138017853,"d":"9.16E+01"}]
[null,"QEP Prescalar",128,"QCAPCTL.CCPS","Capture clock prescaler to 1/128"]
[null,"CAP Count value at MAX freq(Freq Scalar)",234,"freqScaler_pr"]
[]
["100 MHz"]
[null,"CPU Freq",{"v":100000000,"d":"1.00E+08"},null,null,"Inputs"]
[null,"Maximum Required Freq",{"v":10000,"d":"1.00E+04"},"BaseFreq",null,"Output information needed for configuration"]
[null,"Minimum Required Freq",50,null,null,"Information"]
[]
["FREQ_UTIME","Freq measurement rate (Hz)",100,"UTPRD","Unit Time period to be programmed for100Hz"]
[null,"Freq Resolution",50]
[null,"QEP Count at Max Freq",{"v":200,"d":"2.00E+02"},"freqScalar_fr"]
[]
["FREQ_PRD","QEP edges for avg time measurement(2^k)",8,"QCAPCTL.UPPS","Unit position prescalar to 1/8"]
[null,"Time for selected QEP edges at min RPM(s)",0.08,"T= edges/(2*Fmin)"]
[null,"QEP CAP clock to avoid overflow(Hz)",819188,"Fcapmax=maxcnt/T"]
[null,"Minimum QEP Clock pre-scalar",{"v":122.07210066553709,"d":"1.22E+02"}]
[null,"QEP Prescalar",128,"QCAPCTL.CCPS","Capture clock prescaler to 1/128"]
[null,"CAP Count value at MAX freq(Freq Scalar)",313,"freqScaler_pr"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}