{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"flags":["formulas_cached_only"]}
["150 MHz"]
[null,"CPU Freq",{"v":150000000,"d":"1.50E+08"},null,null,"Inputs"]
[null,"Encoder Resolution (4xQEP Lines)",4000,null,null,"Output information needed for configuration"]
[null,"Maximum Required Speed (RPM)",6000," BaseRpm",null,"Information"]
[null,"Minimum Required Speed (Rpm)",10]
[]
["SPEED_FREQ","Speed measurement rate (Hz)",100,"UTPRD","Unit Time period to be programmed for100Hz"]
[null,"Speed Resolutions(Rpm)",1.5]
[]
["SPEED_PRD","QEP edges for avg time measurement(2^k)",32,"QCAPCTL.UPPS","Unit position prescalar to 1/32"]
[null,"Time for selected QEP edges at min RPM(s)",0.048,"T=(edgecnt/enc_resol)* (fmin_prd)","Time it takes 32 edges to occur"]
[null,"QEP CAP clock to avoid overflow(Hz)",1365313,"QPOSCNTmax/T"]
[null,"Minimum QEP Clock pre-scalar",{"v":109.8649174218659,"d":"1.10E+02"},"SYSCLKOUT/CAPCLK"]
[null,"QEP Prescalar",128,"QCAPCTL.CCPS","Capture clock prescaler to 1/128"]
[null,"CAP Count value at MAX speed(Speed Scalar)",94,"SpeedScaler"]
[]
[]
["100 MHz"]
[null,"CPU Freq",{"v":100000000,"d":"1.00E+08"},null,null,"Inputs"]
[null,"Encoder Resolution (4xQEP Lines)",4000,null,null,"Output information needed for configuration"]
[null,"Maximum Required Speed (RPM)",6000," BaseRpm",null,"Information"]
[null,"Minimum Required Speed (Rpm)",10]
[]
["SPEED_FREQ","Speed measurement rate (Hz)",100,"UTPRD","Unit Time period to be programmed for100Hz"]
[null,"Speed Resolutions(Rpm)",1.5]
[]
["SPEED_PRD","QEP edges for avg time measurement(2^k)",32,"QCAPCTL.UPPS","Unit position prescalar to 1/32"]
[null,"Time for selected QEP edges at min RPM(s)",0.048,"T=(edgecnt/enc_resol)* (fmin_prd)","Time it takes 32 edges to occur"]
[null,"QEP CAP clock to avoid overflow(Hz)",1365313,"QPOSCNTmax/T"]
[null,"Minimum QEP Clock pre-scalar",{"v":73.24327828124393,"d":"7.32E+01"},"SYSCLKOUT/CAPCLK"]
[null,"QEP Prescalar",128,"QCAPCTL.CCPS","Capture clock prescaler to 1/128"]
[null,"CAP Count value at MAX speed(Speed Scalar)",63,"SpeedScaler"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}